| VELOSTER(FS) >2012 > G 1.6 GDI > Heating,Ventilation, Air Conditioning > Air Conditioning System > A/C Pressure Transducer>Repair procedures |

Inspection
1. | Measure the pressure of high pressure line by measuring voltage output between NO.1 and NO.2 terminals.
2. | Inspect the voltage value whether it is sufficient to be regular value or not.
Voltage = 0.00878835 * Pressure + 0.5
3. | If the measured voltage value is not specification, replace the A/C pressure transducer.
Replacement
1. | Disconnect the negative (-) battery terminal.
2. | Recover the refrigerant with a recovery/charging station.
3. | Remove the A/C pressure transducer (B) after disconnecting the connector (A).
Tightening torque: 10~12 N.m (1.02~1.22 kgf.m, 7.4~8.8 lb-ft)
Take care that liquid & suction pipe are not bent.
4. | Installation is the reverse order of removal.