| VELOSTER(FS) >2012 > G 1.6 GDI > Steering System > Steering wheel>Repair procedures |

Removal
1. | Disconnect the battery negative cable from the battery and then wait for at least 30 seconds.
2. | Turn the steering wheel so that the front wheels can face straight ahead.
3. | Loosen the bolt (A) and then disconnect the airbag module from the steering wheel.
4. | Disconnect the airbag module connector (A) & horn connector (B) and then remove the airbag module (C) from the steering wheel.
5. | Disconnect the connector (B) & lock nut (A) and then remove the steering wheel by using special service tools (09561-11001).
Tightening torque : 39.2 ~ 49.0N.m(4.0 ~ 5.0kgf.m, 28.9 ~ 36.2lb-ft)
Do not hammer on the steering wheel to remove it. it may damage the steering column.
6. | Installation is the reverse of the removal.
Disassembly
1. | Loosen the screw and then saperate the lower cover (A) from the steering wheel body.
2. | Disconnect the paddle shift connector (A) and then remove lower cover (B).
3. | Remove the paddle shift (A).
4. | Disconnect the all connector and then remove the wiring (A).
5. | Loosen the screw and then remove the remote control switch assembly (A).
6. | Reassemble is the reverse of the disassemble.
Inspection
1. | Check the strain of steering wheel body.
2. | Check the status of the wire to short and open circuit.