| VELOSTER(FS) >2012 > G 1.6 GDI > Body Electrical System > Immobilizer System > Antenna Coil>Repair procedures |

Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the crash pad lower panel. (Refer to the BD group - "Crash pad")
3. | Disconnect the 6P connector (B) after loosening the screw and then remove the antenna coil (A).
Installation
1. | Install the antenna coil.
2. | Connect the antenna coil connector.
3. | Install the crash pad lower panel.