| VELOSTER(FS) >2012 > G 1.6 GDI > Heating,Ventilation, Air Conditioning > Controller > Heater & A/C Control Unit (Manual)>Repair procedures |

Replacement
1. | Disconnect the negative (-) battery terminal.
2. | Using the screwdriver, remove the center facia panel (A).
3. | Disconnect the center fascia cover panel connectors (A).
4. | After loosening the mounting screws, remove the controller (A).
5. | Installation is the reverse order of removal.