| VELOSTER(FS) >2012 > G 1.6 GDI > Body Electrical System > Smart key System>Repair procedures |

Inspection
Self Diagnosis With GDS Smart key system defects can be quickly diagnosed with the GDS. The GDS operates actuator quickly to monitor, input/output value and self diagnosis. The following three features are major concerns in SMART KEY system.
1. | Concerns in SMART KEY unit input.
2. | Concerns in SMART KEY unit.
3. | Concerns in SMART KEY unit output.
The following three diagnostic solutions are the main solution process to a majority of concerns.
1. | SMART KEY unit Input problem : switch diagnosis
2. | SMART KEY unit problem : communication diagnosis
3. | SMART KEY unit Output problem : antenna and switch output diagnosis
Switch Diagnosis
1. | Connect the cable of GDS to the data link connector in driver side crash pad lower panel, turn the power on GDS.
2. | Select the vehicle model and then SMART KEY system.
3. | Select the "SMART KEY unit".
4. | After IG ON, select the "Current data".
5. | You can see the situation of each switch on the GDS after connecting the "current data" process.
Display | Description
FL Toggle switch | ON : Push button is ON in the driver door handle.
FR Toggle switch | ON : Push button is ON in the assist door handle.
Trunk switch | ON : Trunk button is ON.
Gear P Position | ON : Shift lever is P position.
IGN 1 | ON : IGN switch is IG position.
ACC | ON : IGN switch is ACC position.
Push Knob switch | ON : Push knob switch is ON.
External Buzzer | ON : Buzzer is ON.
Communication Diagnosis With GDS (Self Diagnosis)
1. | Communication diagnosis checks that the each linked components operates normal.
2. | Connect the cable of GDS to the data link connector in driver side crash pad lower panel.
3. | After IG ON, select the "DTC".
Antenna Actuation Diagnosis
1. | Connect the cable of GDS to the data link connector in driver side crash pad lower panel.
2. | After IG ON, select the "ACTUATION TEST".
3. | Set the smart key near the related antenna and operate it with a GDS.
4. | If the LED of smart key is blinking, the smart key is normal.
5. | If the LED of smart key is not blinking, check the voltage of smart key battery.
6. | Antenna actuation
A. | INTERIOR Antenna 1
B. | INTERIOR Antenna 2
C. | Trunk antenna
D. | BUMPER/Antenna
E. | DRV_DR Antenna
F. | AST_DR Antenna
Antenna Status Check
1. | Connect the cable of GDS to the data link connector in driver side crash pad lower panel.
2. | Select the "Antenna Status Check".
3. | After IG ON, select the "Antenna Status Check".
4. | Set the smart key near the related antenna and operate it with a GDS.
5. | If the smart key runs normal , the related antenna, smart key(transmission, reception) and exterior receiver are normal.
6. | Antenna status
A. | INTERIOR Antenna 1
B. | INTERIOR Antenna 2
C. | Trunk antenna
D. | BUMPER/Antenna
E. | DRV_DR Antenna
F. | AST_DR Antenna
Serial Communication Status Check
1. | Connect the cable of GDS to the data link connector in driver side crash pad lower panel.
2. | Select the "Serial Communication Line Check".
3. | After IG ON, select the "Receiver Communication Line Check".
4. | Check the serial communication line with a GDS.
5. | If the smart key runs normal, the communication of smart key unit, exterior receiver are normal.
6. | If the smart key runs abnormal, check the following items.
A. | Disconnection or no response of the exterior receiver communication line.
B. | The exterior receiver communication line disconnection and ground connection.
Interior Antenna Actuation Check
1. | Place the smart key in the following shade area and check the IG ON.
2. | If the ignition is ON, the antenna runs normal.
3. | Check the interior antenna ignition mode.
4. | Place the smart key in the following shade area and actuate the antenna. Check the LED of smart key is blinking.
5. | If the LED of smart key is not blinking, check the antenna in shade area.
FOB Status Check
1. | Connect the cable of GDS to the data link connector in driver side crash pad lower panel.
2. | After IG ON, select the "FOB KEY STATUS INFO".
Smart Key Status Check
1. | Connect the cable of GDS to the data link connector in driver side crash pad lower panel.
2. | After IG ON, select the "SMK STATUS INFO".
Neutralization Status Check
1. | Connect the cable of GDS to the data link connector in driver side crash pad lower panel.
2. | After IG ON, select the "Neutralization mode".
Input Switch List
No | Item name | Unit
1 | SSB switch2 | -
2 | ACC | -
3 | IGN1 | -
4 | Gear 'P' Position | -
5 | Brake switch | -
6 | FL Door Lock Button | -
7 | FR Door Lock Button | -
8 | Trunk Lid switch | -
9 | Battery Voltage | -
10 | Alternator Voltage | -
11 | KEY out Indicator Lamp | -
12 | Immobilizer Lamp | -
13 | External Buzzer | -
Actuator List
No. | Item name | Condition
1 | Immo.indicator Lamp | Ignition switch ON Engine off
2 | External Buzzer | Ignition switch ON Engine off
3 | Interior Antenna 1 Active | Ignition switch ON Engine off
4 | Interior Antenna 2 Active | Ignition switch ON Engine off
5 | Trunk Antenna Active | Ignition switch ON Engine off
6 | Bumper Antenna Active | Ignition switch ON Engine off
7 | DRV DR Antenna Active | Ignition switch ON Engine off
8 | AST DR Antenna Active | Ignition switch ON Engine off