| VELOSTER(FS) >2012 > G 1.6 GDI > Suspension System > Front Suspension System > Front Lower Arm>Repair procedures |

Replacement
1. | Remove the front wheel & tire.
Tightening torque : 88.3 ~ 107.9N.m(9.0 ~ 11.0kgf.m, 65.1 ~ 79.6lb-ft)
Be careful not to damage to the hub bolts when removing the front wheel & tire.
2. | Remove the lower arm (A) from the knuckle by using SST (09568-34000).
Tightening torque : 78.5 ~ 88.3N.m(8.0 ~ 9.0kgf.m, 57.9 ~ 65.1lb-ft)
3. | Loosen the bolts & nuts and then remove the lower arm (A) with the sub frame.
Tightening torque : Front 98.1 ~ 117.7N.m(10.0 ~ 12.0kgf.m, 72.3 ~ 86.8lb-ft)
Tightening torque : Rear 156.9 ~ 176.5N.m(16.0 ~ 18.0kgf.m, 115.7 ~ 130.2lb-ft)
4. | Installation is the reverse of removal.
Inspection
1. | Check the bushing for wear and deterioration.
2. | Check the lower arm for deformation.
3. | Check the all bolts and nuts.