| VELOSTER(FS) >2012 > G 1.6 GDI > Suspension System > Tire Pressure Monitoring System > TPMS Receiver>Description and Operation |

Description
Function
1. | LED control, Vehicle Speed signal enter, Diagnostic function (via HS CAN Communications)
2. | Self Diagnosis / Circuit Check
3. | RF frame receive
4. | Tire air pressure, temperature, acceleration, battery data analysis.
5. | WE sensor ID Auto Learning
Operation
Operating mod
1. | Virgin
A. | Stock status
- | Sensor ID not entered
2. | EOL Test mod
A. | Conversion by Command (LID AA hex)
3. | OFF
A. | IG_OFF
4. | Normal
A. | IG_ON
B. | For the main action
- | LED lights up (pressure drop, MIL at the conditions)
- | Self Diagnosis / Circuit Check,
- | WE sensor monitoring
- | Tire air pressure, temperature data analysis.
- | WE sensor ID learning (IG_OFF -> IG_ON, driving over 26km/h during about 19 minutes.