| VELOSTER(FS) >2012 > G 1.6 GDI > Fuel System > General Information>Specifications |

Specifications
Fuel Delivery System
Items | Specification
Fuel Tank | Capacity | 50 lit. (13.2 U.S.gal., 52.8 U.S.qt., 43.9 Imp.qt.)
Fuel Filter | Type | Paper type
Fuel Pressure | Low Pressure Fuel Line | 480 ~ 500 kPa (4.9 ~ 5.1 kgf/cm², 69.6 ~ 72.5 psi)
High Pressure Fuel Line | 2.0 ~ 15.0 MPa (20.4 ~ 153.0 kgf/cm², 290.1 ~ 2175.6 psi)
Fuel Pump | Type | Electrical, in-tank type
Driven by | Electric motor
High Pressure Fuel Pump | Type | Mechanical type
Driven by | Camshaft
Sensors
Manifold Absolute Pressure Sensor (MAPS) ▷ Type: Piezo-resistive pressure sensor type ▷ Specification
Pressure [kPa (kgf/cm², psi)] | Output Voltage (V)
20.0 (0.20, 2.9) | 0.79
46.7 (0.47, 6.77) | 1.84
101.3 (1.03, 14.7) | 4.0
Intake Air Temperature Sensor (IATS) ▷ Type: Thermistor type ▷ Specification
Temperature | Resistance (kΩ)
°C | °F
-40 | -40 | 40.93 ~ 48.35
-20 | -4 | 13.89 ~ 16.03
0 | 32 | 5.38 ~ 6.09
10 | 50 | 3.48 ~ 3.90
20 | 68 | 2.31 ~ 2.57
40 | 104 | 1.08 ~ 1.21
50 | 122 | 1.56 ~ 1.74
60 | 140 | 0.54 ~ 0.62
80 | 176 | 0.29 ~ 0.34
Engine Coolant Temperature Sensor (ECTS) ▷ Type: Thermistor type ▷ Specification
Temperature | Resistance (kΩ)
°C | °F
-40 | -40 | 48.14
-20 | -4 | 14.13 ~ 16.83
0 | 32 | 5.79
20 | 68 | 2.31 ~ 2.59
40 | 104 | 1.15
60 | 140 | 0.59
80 | 176 | 0.32
Throttle Position Sensor (TPS) [integrated into ETC module] ▷ Type: Hall IC Non-contact sensor type ▷ Specification
Throttle angle(°) | Output Voltage (V)
TPS1 | TPS2
0 | 0.5 | 4.5
10 | 0.96 | 4.05
20 | 1.41 | 3.59
30 | 1.87 | 3.14
40 | 2.32 | 2.68
50 | 2.78 | 2.23
60 | 3.23 | 1.77
70 | 3.69 | 1.32
80 | 4.14 | 0.86
90 | 4.6 | 0.41
98 | 4.65 | 0.35
C.T (0) | 0.5 | 4.5
W.O.T (86) | 4.41 | 0.59
Crankshaft Position Sensor (CKPS) ▷ Type: Magnetic field sensitive Type ▷ Specification
Item | Specification
Coil Resistance (Ω) | 774 ~ 946 [20°C (68°F)]
Camshaft Position Sensor (CMPS) ▷ Type: Hall effect type Knock Sensor (KS) ▷ Type: Piezo-electricity type ▷ Specification
Item | Specification
Capacitance (pF) | 950 ~ 1,350
Resistance(MΩ) | 4.87
Heated Oxygen Sensor (HO2S) [Bank 1/Sensor 1] ▷ Type: Zirconia (ZrO2) [Linear] Type ▷ Specification
Item | Specification
Heater Resistance (Ω) | 2.4 ~ 4.0 [20°C(69.8°F)]
Heated Oxygen Sensor (HO2S) [Bank 1/Sensor 2] ▷ Type: Zirconia (ZrO2) [Binary] Type ▷ Specification
A/F Ratio (λ) | Output Voltage(V)
RICH | 0.6 ~ 1.0
LEAN | 0 ~ 0.4
Item | Specification
Heater Resistance (Ω) | Approx. 9.0 [21°C(69.8°F)]
Rail Pressure Sensor (RPS) ▷ Type: Piezo-electricity type ▷ Specification Accelerator Position Sensor (APS) ▷ Type: Variable resistor type ▷ Specification
Accelerator Position | Output Voltage (V)
APS1 | APS2
C.T | 0.7 ~ 0.8 | 0.29 ~ 0.46
W.O.T | 3.85 ~ 4.35 | 1.93 ~ 2.18
Fuel Tank Pressure Sensor (FTPS) ▷ Type: Piezo - Resistivity type ▷ Specification
Pressure [kPa (kgf/cm², in H2O) | Output Voltage (V)
-6.67 (-0.068, -26.8) | 0.5
0 | 2.5
+6.67 (0.068, 26.8) | 4.5
Actuators
Injector ▷ Specification
Item | Specification
Coil Resistance (Ω) | 1.5 [20°C(68°F)]
ETC Motor [integrated into ETC Module] ▷ Specification
Item | Specification
Coil Resistance (Ω) | 0.3 ~ 100 [20°C(68°F)]
Purge Control Solenoid Valve (PCSV) ▷ Specification
Item | Specification
Coil Resistance (Ω) | 22.0 ~ 26.0 [20°C(68°F)]
CVVT Oil Control Valve (OCV) ▷ Specification
Item | Specification
Coil Resistance (Ω) | 6.9 ~ 7.9 [20°C(68°F)]
Variable Intake Solenoid (VIS) Valve ▷ Specification
Item | Specification
Coil Resistance (Ω) | 30.0 ~ 35.0 [20°C(68°F)]
Fuel Pressure Regulator Valve ▷ Specification
Item | Specification
Coil Resistance (Ω) | 0.5 [20°C(68°F)]
Ignition Coil ▷ Type: Stick type ▷ Specification
Item | Specification
Primary Coil Resistance (Ω) | 0.75 ± 15％[20°C(68°F)]
Secendary Coil Resistance (kΩ) | 5.9 [20°C(68°F)]
Canister Close Valve (CCV) ▷ Specification
Item | Specification
Coil Resistance (Ω) | 19.5 ~ 22.5 [20°C(68°F)]
Service Standard
Item | Specification
Ignition Timing (°) | BTDC 5 ± 10
Idle Speed (rpm) | A/C OFF | Neutral, N, P-range | 630 ± 100
D-range | 630 ± 100
A/C ON | Neutral, N, P-range | 700 ± 100
D-range | 700 ± 100
Tightening Torques
Engine Control System
Item | kgf.m | N.m | lb-ft
ECM installation nut | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
ECM bracket installation bolt/nut | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.
Manifold absolute pressure sensor installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Engine Coolant Temperature Sensor installation | 3.0 ~ 4.0 | 29.4 ~ 39.2 | 21.7 ~ 28.9
Crankshaft position sensor installation bolt | 0.8 ~ 1.2 | 7.8 ~ 11.8 | 5.8 ~ 8.7
Camshaft position sensor (Bank 1 / Intake) installation bolt | 0.8 ~ 1.2 | 7.8 ~ 11.8 | 5.8 ~ 8.7
Camshaft position sensor (Bank 1 / Exhaust) installation bolt | 0.8 ~ 1.2 | 7.8 ~ 11.8 | 5.8 ~ 8.7
Knock sensor installation bolt | 1.9 ~ 2.5 | 18.6 ~ 24.5 | 13.7 ~ 18.1
Heated oxygen sensor (Bank 1 / sensor 1) installation | 4.0 ~ 5.0 | 39.2 ~ 49.1 | 28.9 ~ 36.2
Heated oxygen sensor (Bank 1 / sensor 2) installation | 4.0 ~ 5.0 | 39.2 ~ 49.1 | 28.9 ~ 36.2
Rail pressure sensor installation | 3.0 ~ 3.5 | 29.4 ~ 34.3 | 21.7 ~ 25.3
Electronic throttle body installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Purge control solenoid valve bracket installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
CVVT oil control valve (Bank 1 / Intake) installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
CVVT oil control valve (Bank 1 / Exhaust) installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Ignition coil installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Fuel Delivery System
Item | kgf.m | N.m | lb-ft
Fuel tank installation nut | 4.0 ~ 5.5 | 39.2 ~ 54.0 | 28.9 ~ 39.8
Fuel pump plate cover installation bolt | 0.2 ~ 0.3 | 2.0 ~ 2.9 | 1.4 ~ 2.2
Filler-neck assembly bracket installation bolt | 0.8 ~ 1.2 | 7.8 ~ 11.8 | 5.8 ~ 8.7
Filler-neck assembly installation bolt | 0.8 ~ 1.2 | 7.8 ~ 11.8 | 5.8 ~ 8.7
Accelerator pedal module installation nut | 1.0 ~ 1.5 | 9.8 ~ 14.7 | 7.2 ~ 10.8
Accelerator pedal module installation bolt | 0.9 ~ 1.4 | 8.8 ~ 13.7 | 6.5 ~ 10.1
Delivery pipe installation bolt | 1.9 ~ 2.4 | 18.6 ~ 23.5 | 13.7 ~ 17.4
High pressure fuel pump installation bolt | 1.3 ~ 1.5 | 12.8 ~ 14.7 | 9.4 ~ 10.9
High pressure fuel pipe installation nut | 2.7 ~ 3.3 | 26.5 ~ 32.4 | 19.5 ~ 23.9
High pressure fuel pipe function block installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7