| VELOSTER(FS) >2012 > G 1.6 GDI > Manual Transaxle System > Manual Transaxle System>Repair procedures |

Inspection
Manual Transaxle Oil Inspection
1. | Park the vehicle on a level ground and stop the engine.
2. | Retighten the oil filler plug (A) with a new washer.
3. | Check level with finger.
Oil level must be up to fill the hole, if not, add oil until it runs over.
4. | Install the filler plug with a new gasket.
Tightening torque: 58.9 ~ 78.5 N.m (6.0 ~ 8.0 kgf.m, 43.4 ~ 57.8 lb-ft)
Manual Transaxle Oil Replacement
1. | Park the vehicle on a level ground and stop the engine.
2. | Drain the manual transaxle oil after loosening the drain plug (A).
3. | Intall the drain plug with a new gasket
Tightening torque: 58.9 ~ 78.5 N.m (6.0 ~ 8.0 kgf.m, 43.4 ~ 57.9 lb-ft)
4. | Add new oil through the filler plug hole and, fill it just below the plug opening.
Standard oil: SAE 75W/85, API GL-4 Oil capacity: 1.8 ~ 1.9L (0.48 ~ 0.50 U.S.gal., 1.90 ~ 2.01 U.S. qt., 1.58 ~ 1.67 lmp qt.)