| VELOSTER(FS) >2012 > G 1.6 GDI > Body Electrical System > Lighting System > Rear combination lamp>Repair procedures |

Removal
Rear Combination lamp
1. | Disconnect the negative (-) battery terminal.
2. | Disconnect the connector (B) after loosening 2 screws, and then remove the rear combination lamp (A).
3. | Remove the bulb after turning in the counterclockwise direction. A : Side marker lamp B : Tail lamp/ Stop lamp C : Back up lamp D : Turn signal lamp
Installation
1. | Install the rear combination lamp assembly.
2. | Connect the rear combination lamp assembly connector.
3. | Connect the negative (-) battery terminal.