| VELOSTER(FS) >2012 > G 1.6 GDI > Body Electrical System > Back view camera System>Repair procedures |

Removal
Back View Camera
1. | Disconnect the negative(-) battery terminal.
2. | Remove the tailgate outside handle assembly. (Refer to the BD group - "Tailgate")
3. | Disconnect the rear view camera connector (A) after loosening 2 screws.
Installation
1. | Install the tailgate outside handle assembly with the rear view camera.
2. | Install the tailgate outside handle assembly.