| VELOSTER(FS) >2012 > G 1.6 GDI > Driveshaft and axle > General Information>Specifications |

Specification
Engine & T/M | Joint type | Max. permissible angle
Outer | Inner | Outer | Inner
Gamma 1.6 GDI MT | BJ#22 | TJi#22 | 46.5 ° | 23 °
Gamma 1.6 GDI AT | BJ#23 | TJi#22 | 46.5 ° | 23 °
Gamma 1.6 DCT | BJ#22 | TJi#22 | 46.5 ° | 23 °
Tightening torque
Item | N.m | kgf.m | lb-ft
Front | Wheel Hub nuts | 88.2 ~ 107.8 | 9.0 ~ 11.0 | 65.0 ~ 79.5
Driveshaft caulking nut | 196.1 ~ 274.5 | 20.0 ~28.0 | 144.6 ~ 202.5
Strut assembly to knuckle | 137.3 ~ 156.9 | 14.0 ~ 16.0 | 101.3 ~ 115.7
Lower arm to knuckle | 78.5 ~ 88.3 | 8.0 ~ 9.0 | 57.9 ~ 65.1
Tie rod end castle nut | 23.5 ~ 33.3 | 2.4 ~ 3.4 | 19.4 ~ 24.5
Front caliper to knuckle | 78.4 ~ 98.0 | 8.0 ~ 10.0 | 57.8 ~ 72.3
Disc fixing screw | 4.9 ~ 5.8 | 0.5 ~ 0.6 | 3.6 ~ 4.3
Wheel speed sensor & bracket | 7.8 ~ 11.8 | 0.8 ~ 1.2 | 5.8 ~ 8.7
Rear | Wheel Hub nuts | 88.2 ~ 107.8 | 9.0 ~ 11.0 | 65.0 ~ 79.5
Rear caliper mounting bolt | 63.7 ~ 73.5 | 6.5 ~ 7.5 | 47.0 ~ 54.2
Rear axle to torsion beam axle | 49.0 ~ 58.8 | 5.0 ~ 6.0 | 36.1 ~ 43.3
Disc fixing screw | 4.9 ~ 5.8 | 0.5 ~ 0.6 | 3.6 ~ 4.3
Wheel speed sensor & bracket | 4.9 ~ 5.9 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Replace self-locking nuts with new ones after removal.
Lubricants
Joint type | Lubricants | Quantity
BJ#22 | RBA | 90g
BJ#23 | RBA | 90g
TJi#22 | CW09 – VX21 | 135g