| VELOSTER(FS) >2012 > G 1.6 GDI > Body Electrical System > AVN System > AVN Head Unit>Repair procedures |

Removal
AVN Head Unit
• | Take care not to scratch the center fascia panel and related parts.
• | Eject all the disc before removing the AVN head unit to prevent damaging the CD player's load mechanism.
1. | Disconnect the negative (-) battery terminal.
2. | Remove the center fascia panel (A).
3. | Disconnect the connectors (A) from center fascia panel.
4. | Remove the AVN head unit assembly (A), after loosening the 4 screws.
5. | Disconnect the AVN head unit connectors and antenna cables (A), then remove the AVN head unit.
If the CD does not eject, do not attempt to remove it because the audio unit may be damaged.Contact an authorized hyundai dealership for assistance.
External Amplifier
1. | Remover the assistant seat. (Refer to the BD group - "Seat - Front seat")
2. | Disconnect the external amplifier connector.
3. | Loosen a bolt and 3 nuts, then remove the external amplifier (A).
Installation
AVN Head Unit
1. | Connect the AVN head unit connectors and cables.
2. | Install the AVN head unit.
3. | Install the center fascia upper panel.
4. | Connect the negative (-) battery terminal.
Make sure the AVN head unit connectors are plugged in properly and the antenna cable is connected properly.
External Amplifier
1. | Connect the connector and install the external amplifier.
2. | Install the assistant seat.