| VELOSTER(FS) >2012 > G 1.6 GDI > Engine Electrical System > Charging System>Description and Operation |

Description
The charging system includes a battery, an alternator with a built-in regulator, and the charging indicator light and wire. The Alternator has built-in diodes, each rectifying AC current to DC current. DC current appears at alternator "B" terminal. The charging voltage of this alternator is regulated by the battery voltage detection system (or ECM - with AMS). The main components of the alternator are the rotor, stator, rectifier, capacitor, brushes, bearings and V-ribbed belt pulley (or OAD : Overrunning Alternator Decoupler). The brush holder contains a built-in electronic voltage regulator.
1. Brush 2. Drive belt pulley 3. Rotor 4. Stator 5. Rectifier
Alternator Management System (AMS) Alternator management system controls the charging voltage set point in order to improve fuel economy, manage alternator load under various operating conditions, keep the battery charged, and protect the battery from over-charging. ECM controls generating voltage by duty cycle (charging control, discharging control, normal control) based on the battery conditions and vehicle operating conditions. The system lowers the charging rate when accelerating. Lowering the charging rate will allow more engine power for accelerating. The system increases the charging rate when decelerating. The system uses the unused power of the decelerating engine and increases the charging rate.