| VELOSTER(FS) >2012 > G 1.6 GDI > Fuel System > Engine Control System > Fuel Pressure Control Valve>Repair procedures |

Inspection
1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.
2. | Disconnect the fuel pressure regulator valve connector.
3. | Measure resistance between the fuel pressure regulator valve terminals 1 and 2.
4. | Check that the resistance is within the specification.
Specification: Refer to “Specification”