| VELOSTER(FS) >2012 > G 1.6 GDI > Heating,Ventilation, Air Conditioning > Air Conditioning System > Refrigerant line>Repair procedures |

Replacement
1. | Discharge refrigerant from refrigeration system.
2. | Replace faulty tube or hose.
Cap the open fittings immediately to keep moisture or dirt out of the system.
3. | Tighten joint of bolt or nut to specified torque.
Connections should not be torque tighter than the specified torque.
Part tightened | N.m | Kgf.m | lbf.ft
Condenser - Discharge hose | 4.9~7.8 | 0.5~0.8 | 3.6~5.8
Condenser - Liquid tube
Compressor - Discharge hose | 18.6~27.4 | 1.9~2.8 | 13.7~20.2
Compressor - Suction hose
Expansion valve - Evaporator | 6.9~10.8 | 0.7~1.1 | 5.1~8.0
4. | Evacuate air in refrigeration system and charge system with refrigerant.
Specified amount : 420 ± 25g (14.8±0.88 oz.)
5. | Inspect for leakage of refrigerant. Using a gas leak detector, check for leakage of refrigerant.
6. | Inspect A/C operation.