| VELOSTER(FS) >2012 > G 1.6 GDI > Body Electrical System > BCM (Body Control Module) > IPM (Intelligent integrated Platform Module)>Repair procedures |

Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the crash pad lower panel. (Refer to the BD group - "Crash pad")
3. | Disconnect the IPM connectors, loosening the nut (2EA) and the bolt (1EA), then remove the IPM.
4. | The installation is the reverse order of removal.
IPM Diagnosis with GDS
1. | It will be able to diagnose defects of IPM with GDS quickly. GDS can operates actuator manually, input/output value monitoring and self diagnosis.
2. | Select model and "IPM".
3. | Select the module to check.
4. | Select "Input/output monitoring", if you will check current data of body network system. It provides input/output status of each module.
5. | If you will check each module data operation manually, select "Actuation test".
6. | To check the DTC of the each module, select "DIAGNOSTIC TROUBLE CODES".
7. | If you want to change user option, select “user option”.