| VELOSTER(FS) >2012 > G 1.6 GDI > Driveshaft and axle > Rear Axle Assembly > Rear Hub - Carrier>Repair procedures |

Replacement
1. | Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported.
2. | Remove the rear wheel and tire (A) from rear hub .
Tightening torque: 88.2 ~ 107.8 N.m (9.0 ~ 11.0 kgf.m, 65.0 ~ 79.5 lb-ft)
Be careful not to damage to the hub bolts when removing the rear wheel and tire (A).
3. | Remove the clip (A) and then remove the parking brake cable (B).
4. | Remove the brake caliper mounting bolts, and then place the brake caliper assembly (A) with wire.
Tightening torque: 63.7 ~ 73.5 N.m (6.5 ~ 7.5 kgf.m, 47.0 ~ 54.2 lb-ft)
5. | Loosen the mounting screws and then brake disc (A).
Tightening torque: 4.9 ~ 5.8 N.m (0.5 ~ 0.6 kgf.m, 3.6 ~ 4.3 lb-ft)
6. | Loosen the hub mounting bolt and then remove the hub (A) from torsion beam axle.
Tightening torque: 49.0 ~ 58.8 N.m (5.0 ~ 6.0 kgf.m, 36.1 ~ 43.3 lb-ft)
7. | Install in the reverse order of removal.
Inspection
1. | Check the hub for cracks and the splines for wear.
2. | Check the brake disc for scoring and damage.
3. | Check the rear axle carrier for cracks
4. | Check the bearing for cracks or damage.