| VELOSTER(FS) >2012 > G 1.6 GDI > Steering System > General Information>Specifications |

Specifications
Item | Specification
Type | Electric Power Steering System
Steering gear | Type | Rack & Pinion
Rack stroke | 150mm (5.90in.)
Steering angle (Max.) | Inner | 39.9° ± 1.5°
Outer | 32.8°
Tightening Torques
Item | Tightening torque (kgf.m)
Nm | kgf.m | lb-ft
Wheel Hub nuts | 88.3 ~ 107.9 | 9.0 ~ 11.0 | 65.1 ~ 79.6
Steering wheel lock nut | 39.2 ~ 49.0 | 4.0 ~ 5.0 | 28.9 ~ 36.2
Steering column & universal joint | 53.9 ~ 63.7 | 5.5 ~ 6.5 | 39.8 ~ 47.0
Steering column mounting nuts | 12.7 ~ 17.7 | 1.3 ~ 1.8 | 9.4 ~ 13.0
Steering column mounting bolt | 44.1 ~ 49.0 | 4.5 ~ 5.0 | 32.5 ~ 36.2
Universal joint to pinion | 32.4 ~ 38.3 | 3.3 ~ 3.8 | 23.9 ~ 27.5
Tie rod end castle nut | 23.5 ~ 33.3 | 2.4 ~ 3.4 | 17.4 ~ 24.6
Lower arm to front axle | 78.5 ~ 88.8 | 8.0 ~ 9.0 | 57.9 ~ 65.1
Steering gear box to sub frame | 58.8 ~ 78.5 | 6.0 ~ 8.0 | 43.4 ~ 57.9
Stabilizer link nut | 98.1 ~ 117.7 | 10.0 ~ 12.0 | 72.3 ~ 86.8
Sub frame mounting bolts & nuts | 156.9 ~ 176.5 | 16.0 ~ 18.0 | 115.7 ~ 130.2
Sub frame stay bolts | 44.1 ~ 53.9 | 4.5 ~ 5.5 | 32.5 ~ 39.8