| VELOSTER(FS) >2013 > G 1.6 GDI > Body (Interior and Exterior) > Interior > Interior Trim>Repair procedures |

Replacement
Door Scuff Trim Replacement
• | Put on gloves to protect your hands.
• | Use a plastic panel removal tool to remove interior trim pieces to without marring the surface.
• | Take care not to bend or scratch the trim and panels.
1. | Using a screwdrier or remover, remove the front door scuff trim (A). [Front]
2. | Remove the rear seat cushion. (Refer to the BD group - "Rear Seat")
3. | After loosening the mounting screw, then remove the rear door scuff trim (A). [Rear]
4. | Installation is the reverse of removal.
• | Replace any damage clips.
Front Pillar Trim Replacement
• | Put on gloves to protect your hands.
• | Use a plastic panel removal tool to remove interior trim pieces to without marring the surface.
• | Take care not to bend or scratch the trim and panels.
1. | Using a screwdriver or remover, remove the front pillar trim (A).
2. | Installation is the reverse of removal.
• | Replace any damage clips.
Cowl Side Trim Replacement
• | Put on gloves to protect your hands.
• | Use a plastic panel removal tool to remove interior trim pieces to without marring the surface.
• | Take care not to bend or scratch the trim and panels.
1. | Remove the front door scuff trim.
2. | Remove the hood latch release handle. (Refer to the BD group - "Hood")
3. | Using a screwdriver or remover, remove the cowl side trim (A).
• | Be careful not to damage the cowl side trim clip (B).
• | Pull the cowl side tirm as direction of the arrow and then remove the tirm.
4. | Installation is the reverse of removal.
• | Replace any damage clips.
Center Pillar Trim Replacement
• | Put on gloves to protect your hands.
• | Use a plastic panel removal tool to remove interior trim pieces to without marring the surface.
• | Take care not to bend or scratch the trim and panels.
1. | Remove the following items first :
A. | Front door scuff trim (Refer to the BD group – “Interior Trim”).
B. | Rear door scuff trim [RH] (Refer to the BD group – “Interior Trim”).
2. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.
3. | The seat belt anchor pretensioner (A) be removed after pushing the lock pin (B) as arrow direction. [LH] [RH]
4. | Using a screwdriver or remover, remove the center pillar lower trim (A). [LH] [RH]
5. | Using a screwdriver or remover, remove the front seat belt upper anchor cover (A). [LH] [RH]
6. | After loosening the mounting bolt, then remove the front seat belt upper anchor (A). [LH]
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
[RH]
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
7. | After loosening the mounting bolt, then remove the center pillar upper trim (A). [LH] [RH]
8. | Installation is the reverse of removal.
• | Replace any damage clips.
Rear Pillar Trim Replacement
• | Put on gloves to protect your hands.
• | Use a plastic panel removal tool to remove interior trim pieces to without marring the surface.
• | Take care not to bend or scratch the trim and panels.
1. | Remove the rear seat. (Refer to the BD group – “Rear Seat”)
2. | Using a screwdriver or remover, remove the rear transverse trim (A).
3. | After loosening the mounting screw, then remove the rear door scuff trim (A).
4. | After loosening the mounting bolt, then remove the rear seat belt lower anchor (A). [LH, RH]
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
5. | Using a screwdriver or remover, remove the center pillar lower trim (A). [LH]
6. | Using a screwdriver or remover, remove the luggage side trim lamp (A).
7. | Disconnect the luggage side trim lamp connector (B).
8. | After loosening the mounting screws, then remove the luggage side trim (C). [LH] [RH]
9. | After loosening the mounting bolts, then remove the rear pillar trim (A). [LH] [RH]
10. | Installation is the reverse of removal.
• | Replace any damage clips.
• | Make sure the connector is connected properly.
Luggage Side Trim Replacement
• | Put on gloves to protect your hands.
• | Use a plastic panel removal tool to remove interior trim pieces to without marring the surface.
• | Take care not to bend or scratch the trim and panels.
1. | Remove the following items first :
A. | Rear seat assembly (Refer to the BD group - "Rear Seat")
B. | Front door scuff trim [LH]
C. | Center pillar lower trim [LH]
D. | Rear door scuff trim [RH]
E. | Rear transverse trim
2. | After loosening the mounting screws, then remove the luggage side trim.
3. | Installation is the reverse of removal.
• | Replace any damage clips.
1. Luggage side trim [RH] 2. Luggage side trim [LH] 3. Rear pillar trim [RH] 4. Rear pillar trim [LH] 5. Luggage rear cover [RH] 6. Luggage rear cover [LH] | 7. Rear transverse trim 8. Luggage net assembly 9. Load floor front trim 10. Luggage covering mat 11. Car warning triangle assembly 12. C piller shelf center trim