| VELOSTER(FS) >2013 > G 1.6 GDI > Clutch System > Clutch System > Clutch Release Cylinder>Repair procedures |

Removal
1. | Drain the brake fluid through the bleed plug (A).
2. | Remove the clutch release cylinder assembly (C) after removing thd tube (B) and nuts (A-2ea).
Tightening torque: 14.7 ~ 21.6 N.m (1.5 ~ 2.2 kgf.m, 10.9 ~ 15.9 lb-ft)
Installation
1. | Installation is the reverse of removal.
Coat the clutch clevis push rod specified grease.
Specified grease: CASMOLY L9508
Adjustment
Clutch Release Cylinder Air Bleeding Procedure
Use the specified fluid. Avoid mixing different brands of fluid.
Specified fluid: SAE J1703 (DOT 3 or DOT 4)
1. | After disconnecting a cap from the clutch release cylinder air bleeder, insert a vinyl hose in the plug.
2. | Loosening the plug screw, press and release the clutch pedal about 10 times.
3. | Tighten the plug (A) during the clutch pedal pressed. Afterwards, raise the pedal with a hand.
4. | After pressing the clutch pedal 3 times more, loosen the plug (A) and retighten it with the pedal pressed. Raise it again, then.
5. | Repeat the step 4 two or three times. (until there is no bubble in the fluid)
Tightening torque: 6.8 ~ 9.8 N.m (0.7 ~ 1.0 kgf.m, 9.2 ~ 13.3 lb-ft)
6. | Refill the clutch master cylinder with the specified fluid.