| VELOSTER(FS) >2013 > G 1.6 GDI > Body Electrical System > Hands Free System > Hands Free Switch>Repair procedures |

Inspection
1. | Check the hands free remote control switch for resistance between terminals in each switch position.
Switch | Connector terminal | Resistance (±5%)
Voice | 3 - 4 | 10.71 kΩ
End of call | 3 - 4 | 18.91 kΩ
Send | 3 - 4 | 40.91 kΩ
Removal
1. | Disconnect the negative(-) battery terminal.
2. | Remove th driver airbag module. (Refer to the RT group - "Driver airbag(DAB) and clock spring)
3. | Remove the steering wheel. (Refer to the ST group - "Steering column and shaft")
4. | Remove the cover(A) after loosening screws.
5. | Disconnector the left audio switch (A).
6. | Disconnector the right hands free switch and trip switch (A).
7. | Remove the wiring (A) then loosening 5 screws.
8. | Remove the steering wheel remote control switchs assembly (A).
Installation
1. | Install the hands free switch to the steering wheel.
2. | Install the steering wheel cover.
3. | Install the steering wheel.
4. | Reassemble the driver airbag module.
Make sure the hands free remote control switch and the airbag module connectors are plugged in properly.