| VELOSTER(FS) >2013 > G 1.6 GDI > Body Electrical System > AVN System > Speakers>Repair procedures |

Inspection
1. | Troubleshooting for Speaker
(1) | Basic inspection of speaker Inspect the sound from speaker after verifying that the speaker mounting screws are removed and the wiring connector is connected to remove any possible vibration transmitted from body trims and surrounding parts.
(2) | Case Troubleshooting
No. | Case | Inspection/Remedy
1 | Trembling sound |
1. | Before replacing the speaker, inspect that the mounting screw is installed normally.
2. | After re-installing the speaker, verify that no trembling sound is heard.
3. | When hearing a trembling sound again, replace the speaker with new one.
2 | Noise |
1. | Check if the wiring connector is connected normally. If not, reconnect the wiring connector.
2. | In case of radio static, check if there is a noise from CD.
3. | If a noise is heard with the radio and CD on, replace the speaker with new one.
In case there is only radio static, this causes from poor radio reception. Thus the speaker needs no repair and replacement.
3 | Speaker inoperative | Inspection of the wiring connection between the battery and the speaker
1. | Before replacing the speaker, inspect the wiring connection between the battery and the speaker is normal.
2. | Check the supply power to the speaker and the resistance, then inspect the sound quality. ■ Specified impedance : 2 ~ 4Ω
3. | If the speaker works poorly, replace it with new one.
When handling the speakers:
- | Do not damage the speaker with impact, like dropping or throwing it.
- | Be careful not to drop water and oil on the speakers.
- | Caution during handling of speaker because the material of diaphragm is paper which is easily torn by impact or external force.
- | Modifying the audio system may cause damage to the speakers. If this is the case, the speakers are not covered by the manufacturer's warranty.
Removal
Front Speaker
1. | Remove the front door trim panel and speaker connector. (Refer to the BD group - "Front door")
2. | Remove the front speaker (A) after loosening 4 rivets.
Rear Speaker (Right)
1. | Remove the rear door trim panel and speaker connector. (Refer to the BD group - "Interior trim")
2. | Remove the rear speaker (A) after removing 4 rivets.
Rear Speaker (Left)
1. | Remove the rear door trim panel and speaker connector. (Refer to the BD group - "Interior trim")
2. | Remove the rear speaker (A) after removing 4 bolts.
Center Speaker
1. | Remove the crash pad upper speaker cover (A).
2. | Disconnect the connector, after loosening 2 screws then remove the center speaker (A).
Midrange Speaker
1. | Remove the front door trim panel and speaker connector. (Refer to the BD group - "Front door")
2. | Remove the front midrange speaker, after loosening 2 screws.
Subwoofer Speaker
1. | Remove the rear fillar trim panel and speaker connector. (Refer to the BD group - "Interior trim")
2. | Remove the subwoofer speaker (A), after loosening 2 bolts and 2 nuts.
Installation
Front Speaker
1. | Install the front speaker.
2. | Insatll the rivets and connect the connector.
3. | Install the front door trim panel.
Rear Speaker (Right)
1. | Install the rear speaker.
2. | Install the rivets and connect the connector.
3. | Install the door trim panel.
Rear Speaker (Left)
1. | Install the rear speaker after connecting the connector.
2. | Install the door trim panel.
Center Speaker
1. | Install the center speaker after connecting the connector.
2. | Install the center speaker cover.
Mindrange Speaker
1. | Install the midrange speaker after connecting the connector.
2. | Install the front door trim panel.
Subwoofer Speaker
1. | Install the subwoofer speaker after connecting the connector.
2. | Install the rear fillar trim panel.