| VELOSTER(FS) >2013 > G 1.6 GDI > Dual Clutch Transmission(DCT) System > Dual Clutch Transmission Control System > Gear Actuator Motor>Repair procedures |

Inspection
1. | Turn off the ignition switch.
2. | Disconnect the gear actuator motor connector.
3. | Measure the resistance on the gear actuator motor terminal.
4. | Refer to the specifications and check that the measured resistance is as specified.
Removal
1. | Remove the gear actuator assembly. (Refer to "Gear actuator" in this group)