| VELOSTER(FS) >2013 > G 1.6 GDI > Dual Clutch Transmission(DCT) System > Dual Clutch Transmission Control System > Shift Lever>Repair procedures |

Removal
1. | Remove the floor console assembly. (Refer to the Interior (Console) of BD Group.)
2. | Disconnect the sports mode connector (A).
3. | Remove the control cable (A).
4. | Remove the bolt and then the shift lever assembly (A).
Tightening torque: 9.8 ~ 14.7 N.m (1.0 ~ 1.5 kgf.m, 7.2 ~ 10.8 lb-ft)
Installation
1. | Installation is the reverse of removal.
Install the cable after placing the shift lever and the transmission manual control lever in the N position.
Changing the Shift Cable
1. | Remove the floor console assembly. (Refer to the Interior (Console) of BD Group.)
2. | Remove the control cable (A).
3. | Remove the retainer (A) and nut (B).
Tightening torque: 11.8 ~ 14.7 N.m (1.2 ~ 1.5 kgf.m, 8.7 ~ 10.8 lb-ft)
4. | Remove the cable (B) from the cable bracket (A) on the A/T.
5. | Remove the nut (C) from the manual control lever.
6. | Remove the shift cable by pulling it toward the interior.
Tightening torque: 9.8 ~ 14.7 N.m (1.0 ~ 1.5 kgf.m, 7.2 ~ 10.8 lb-ft)
7. | Installation is the reverse of removal.
• | Install the cable after placing the shift lever and the transmission manual control lever in the N position.
• | Adjust the control cable. (Refer to the Control Cable Adjustment Procedure.)
Adjustment
Adjusting the Control Cable
1. | Place the shift lever in the interior, and the transmission manual control lever, to the N position.
2. | Connect the shift lever (A) in the interior with the control cable (B).
3. | Lightly push the shift cable towards F to tighten the cable.
4. | Tighten the nut (A) to the specified torque.
Tightening torque: 9.8 ~ 14.7 N.m (1.0 ~ 1.5 kgf.m, 7.2 ~ 10.8 lb-ft)