| VELOSTER(FS) >2013 > G 1.6 GDI > Body Electrical System > Seat Electrical > Power Seat Motor>Repair procedures |

Inspection
Power seat motor
1. | Remove the seat and Lumbar support motor (A) connectors.
2. | With the battery connected directly to the motor terminals, check if the motors run smoothly.
3. | Reverse the connections and check that the motor rotates in reverse.
4. | If there is an abnormality, replace the motor.