| VELOSTER(FS) >2013 > G 1.6 GDI > Fuel System > Fuel Delivery System > Filler-Neck Assembly>Repair procedures |

Removal
1. | Open the fuel filler door, and then remove the filler-neck assembly mounting screws (A).
2. | Disconnect the fuel filler hose (A) and the ventilation hose (B).
3. | Remove the filler-neck assembly from the vehicle after removing the bracket mounting bolt (C).
Installation
1. | Installation is reverse of removal.
Filler-neck assembly bracket installation nut : 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft) Filler-neck assembly installation screw : 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft)