| VELOSTER(FS) >2013 > G 1.6 GDI > Emission Control System > Evaporative Emission Control System > Canister>Repair procedures |

Removal
1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.
2. | Lift the vehicle.
3. | Disconnect the vapor tube quick-connector (A,B) and the ventilation hose (C).
4. | Remove the canister assembly after removing installation bolts (D).
Inspection
1. | Check for the following items visually. - Cracks or leakage of the canister - Loose connection, distortion, or damage of the vapor hose/tube A: Canister ↔ Atmosphere (Fuel tank air filter) B: Canister ↔ Intake manifold C: Canister ↔ Fuel tank
Installation
Installation is the reverse of removal.
Canister bracket installation bolt: 19.6 ~ 29.4 N.m (2.0 ~ 3.0 kgf.m, 14.5 ~ 21.7 lb-ft) Canister installation bolt: 3.9 ~ 5.9 N.m (0.4 ~ 0.6 kgf.m, 2.9 ~ 4.3 lb-ft)