| VELOSTER(FS) >2013 > G 1.6 GDI > Fuel System > Engine Control System > CVVT Oil Control Valve (OCV)>Repair procedures |

Inspection
1. | Turn the ignition switch OFF.
2. | Disconnect the OCV connector.
3. | Measure resistance between the OCV terminals 1 and 2.
4. | Check that the resistance is within the specification.
Specification: Refer to “Specification”
Removal
1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.
2. | Disconnect the CVVT oil control valve connector (A).
3. | Remove the installation bolt (B), and then remove the valve from the engine. [Bank 1 / Intake] [Bank 1 / Exhaust]
Installation
• | Install the component with the specified torques.
• | Note that internal damage may occur when the component is dropped. If the component has been dropped, inspect before installing.
• | Apply engine oil to the valve O-ring.
1. | Installation is reverse of removal.
CVVT oil control valve installation bolt: 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)