| VELOSTER(FS) >2013 > G 1.6 GDI > Dual Clutch Transmission(DCT) System>Specifications |

Specifications
Model | D6GF1
Engine | Gasoline 1.6 GDI
Shift ratio | 1st | 3.615
2nd | 1.955
3rd | 1.303
4th | 0.943
5th | 0.939
6th | 0.743
Reverse | 4.531
Final gear ratio 1 | 4.813
Final gear ratio 2 | 3.667
Sensor
Speed Sensor ▷ Type: Hall effect sensor ▷ Specifications
Item | Specifications
Output voltage (V) | Low | 0.7
High | 1.4
Motor
Clutch Actuator Motor ▷ Specifications
Item | Specifications
Operating condition (°C) °F | (20) 68
Output resistance (mΩ) | 48 ± 7%
Inhibitor Switch
▷ Type: Single signal output type ▷ Specifications
Item | Specifications
Output type | Combined signal output
Input voltage (V) | 12
Tightening torque
Item | N.m | kgf.m | lb-ft
TCM mounting bolt/nut | 9.8 ~ 11.8 | 1.0 ~ 1.2 | 7.2 ~ 8.7
Shift cable bracket bolt | 19.6 ~ 26.5 | 2.0 ~ 2.7 | 14.4 ~ 19.5
Input speed sensor bolt | 7.8 ~ 9.8 | 0.8 ~ 1.0 | 5.7 ~ 7.2
Shift lever assembly bolt | 8.8 ~ 13.7 | 0.9 ~ 1.4 | 6.5 ~ 10.1
Inhibitor switch mounting bolt | 9.8 ~ 11.8 | 1.0 ~ 1.2 | 7.2 ~ 8.7
Oil drain plug | 58.8 ~ 78.4 | 6.0 ~ 8.0 | 43.2 ~ 57.6
Oil level plug | 58.8 ~ 78.4 | 6.0 ~ 8.0 | 43.2 ~ 57.6
Starter motor mounting bolt | 42.2 ~ 53.9 | 4.3 ~ 5.5 | 31.1 ~ 39.8
Transmission upper mounting bolt (transmission => engine) | 42.2 ~ 53.9 | 4.3 ~ 5.5 | 31.1 ~ 39.8
Transmission lower mounting bolt (engine => transmission) | 42.2 ~ 53.9 | 4.3 ~ 5.5 | 31.1 ~ 39.8
Transmission support bracket mounting bolt | 88.3 ~ 107.9 | 9.0 ~ 11.0 | 65.1 ~ 79.6
Lubricant
Item | Specified lubricant | Capacity
Transmission oil | HA SYN MTF (SK) HD SYN MTF (H.K.SHELL) GS PAO MTF (GS CALTEX) HYUNDAI Genuine transaxle (SAE 75W/85, API GL-4) | Approx. 1.9 L (0.50 U.S gal., 2.01 U.S.qt.,1.67 Imp.qt.)