| VELOSTER(FS) >2013 > G 1.6 GDI > Engine Electrical System > General Information>Specifications |

Specifications
Ignition System
Items | Specification
Ignition coil | Primary resistance | 0.75 ± 15% (Ω)
Secondary resistance | 5.9 (kΩ)
Spark plugs | Type | SILZKR6B10
Gap | 0.9 ~ 1.0 mm ( 0.0433 ~ 0.0394 in.)
Starting System
Items | Specification
Starter | Rated voltage | 12 V, 0.9kW
No. of pinion teeth | 8
No-load characteristics | Voltage | 11.5V
Ampere | 60A, MAX
Speed | 5,500rpm, MIN
Charging System
Items | Specifications
Alternator (AMS) | Rate voltage | 13.5V, 90A
Speed in use | 1,000 ~ 18,000 rpm
Voltage regulator | IC regulator built-in type
Regulator setting voltage | External mode | ECU control
Internal mode | 14.55 ± 0.3V
Temperature compensation | External mode | ECU control
Internal mode | -3.5 ± 2mV / °C
Battery | Type | 36-20GL
Cold cranking amperage [at -18°C(-0.4°F)] | 410 A
Reserve capacity | 80 min
Specific gravity [at 25°C(77°F)] | 1.280 ± 0.01
• | COLD CRANKING AMPERAGE is the amperage a battery can deliver for 30 seconds and maintain a terminal voltage of 7.2V or greater at a specified temperature.
• | RESERVE CAPACITY RATING is amount of time a battery can deliver 25A and maintain a minimum terminal voltage of 10.5V at 26.7°C(80.1°F).