| VELOSTER(FS) >2013 > G 1.6 GDI > Emission Control System > General Information>Specifications |

Specifications
Purge Control Solenoid Valve (PCSV) ▷ Specification
Item | Specification
Coil Resistance (Ω) | 22.0 ~ 26.0 [20°C(68°F)]
Fuel Tank Pressure Sensor (FTPS) ▷ Type: Piezo-Resistive Pressure Sensor ▷ Specification
Pressure [kPa (kgf/cm², in H2O)] | Output Voltage (V)
-6.67 (-0.068, -26.8) | 0.5
0 | 2.5
+6.67 (0.068, 26.8) | 4.5
Canister Close Valve (CCV) ▷ Specification
Item | Specification
Coil Resistance (Ω) | 19.5 ~ 22.5 [20°C(68°F)]
Tightening Torques
Item | kgf.m | N.m | lb-ft
Positive crankcase ventilation valve installation | 0.8 ~ 1.2 | 7.8 ~ 11.8 | 5.8 ~ 8.7
Canister bracket installation bolt | 2.0 ~ 3.0 | 19.6 ~ 29.4 | 14.5 ~ 21.7
Canister installation bolt | 0.4 ~ 0.6 | 3.9 ~ 5.9 | 2.9 ~ 4.3
Fuel tank air filter installation bolt | 0.4 ~ 0.6 | 3.9 ~ 5.9 | 2.9 ~ 4.3