| VELOSTER(FS) >2013 > G 1.6 GDI > Body Electrical System > Seat Electrical > Seat Heater>Repair procedures |

Inspection
First Seat Heater
1. | Check for continuity and measure the resistance between terminals. [Cushion]
No. | Description | No. | Description
1 | - | 4 | NTC-
2 | - | 5 | NTC+
3 | Heater(-) | 6 | Heater(+)
Standard value (Fabric / Leather) Cushion : 1.18 Ω ± 10% Back: 1.13 Ω ± 10% Set : 2.31 Ω ± 10%
2. | Operate the seat heater after connecting the connector, and then check the thermostat by measuring the temperature of seat surface.
Standard value (Fabric / Leather) Cushion : High : 42 ± 2°C(107.6 ± 35.6°F) / LOW : 39 ± 2°C(102.2 ± 35.6°F) Back : High : 52 ± 2°C(125.6 ± 35.6°F) / LOW : 46 ± 2°C(114.8 ± 35.6°F)