| VELOSTER(FS) >2013 > G 1.6 GDI > Body (Interior and Exterior) > Body Dimensions > Side Body>Body Repair |

Side Body A (LH)
Front side member tooling hole (Ø12) | Fender apron upper member tooling hole (Ø7) | Front door upper hinge mounting hole (Ø13)
Front door lower hinge mounting hole (Ø13) | Front door switch mounting hole (Ø10) | Quarter fixed glass mounting notch
Rear combination lamp mounting hole (Ø6) | Quarter outer panel corner |
Side Body B (LH)
Side outer panel notch | Side outer panel notch | Side outer panel notch
Side outer panel notch | Front door switch mounting hole (Ø10) |
Side Body C (RH)
Front side member tooling hole (Ø12) | Fender apron upper member tooling hole (Ø7) | Front door upper hinge mounting hole (Ø13)
Front door lower hinge mounting hole (Ø13) | Rear door upper hinge mounting hole (Ø13) | Rear door lower hinge mounting hole (Ø13)
Rear combination lamp mounting hole (Ø6) | Quarter outer panel corner |
Side Body D (RH)
Side outer panel notch | Side outer panel notch | Side outer panel notch
Side outer panel notch | Front door switch mounting hole (Ø10) | Side outer panel notch
Side outer panel notch | Side outer panel notch | Rear door switch mounting hole (Ø10)