| VELOSTER(FS) >2013 > G 1.6 GDI > Body (Interior and Exterior) > Exterior > Cowl Top Cover>Repair procedures |

Replacement
1. | Using a screwdriver or remover, remove the wiper arm cover (A).
2. | Remove the wiper arm mounting hole plug (B).
3. | After loosening the mounting nuts, then remove the wiper arm (A).
Tightening torque : 22.6 ~ 26.5 N.m (2.3 ~ 2.7 kgf.m, 16.6 ~ 19.5 lb-ft)
4. | Remove the washer nozzle hose (B).
5. | Detach the clips, then remove the cowl top cover (A).
6. | Installation is the reverse of removal.
• | Replace any damage clips.