| VELOSTER(FS) >2013 > G 1.6 GDI > Body Electrical System > Rear Parking Assist System > Parking Assist Sensor>Repair procedures |

Removal
1. | Remove the rear bumper. (Refer to the Body group - "Rear bumper")
2. | Disconnect the connector from the rear bumper.
3. | Disconnect the connector(B) from the rear ultra sensor(A).
4. | Pull out the sensor (A) by opening the sensor holder (C) out.
Installation
1. | Install the rear ultra sensor after connecting the connector.
2. | Install the rear bumper.