| VELOSTER(FS) >2013 > G 1.6 GDI > Restraint (Depowered) > Airbag Module > Passenger Airbag (PAB) Module>Repair procedures |

Removal
1. | Disconnect the battery negative cable and wait for at least three minutes before beginning work.
2. | Remove the glove box housing. (Refer to the Body group - "Crash pad")
3. | Disconnect the passenger airbag connector (A) and remove the PAB mounting bolt (B).
4. | Remove the crash pad. (Refer to the Body group - "Crash pad")
Replace the crash pad which is damaged while PAB is deployed.
5. | Remove the mounting bolts from the crash pad. Then remove the passenger airbag.
The removed airbag module should be stored in a clean, dry place with the airbag cushion up.
Installation
1. | Remove the ignition key from the vehicle.
2. | Disconnect the battery negative cable from battery and wait for at least three minutes before beginning work.
3. | Place a passenger airbag on the crash pad and tighten the passenger airbag mounting bolts.
Tightening torque: 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft)
4. | Install the crash pad. (Refer to the Body group - "Crash pad")
5. | Tighten the passenger airbag mounting bolts.
Tightening torque: 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft)
6. | Connect the passenger airbag harness connector to the SRS main harness connector.
7. | Reinstall the glove box housing. (Refer to the Body group - "Crash pad")
8. | Reconnect the battery negative cable.
9. | After installing the passenger airbag (PAB), confirm proper system operation:
A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.