| VELOSTER(FS) >2013 > G 1.6 GDI > Suspension System > Tire Pressure Monitoring System>Troubleshooting |

System self diagnosis
Possible to detect abnormal situations from Sensor data
• | High Temperature – Sensor's temperature is more than 100 °C
• | Battery Low – Sensor's battery is less than 2.1v
• | Sensor Failure
ECU can be detected any abnormal situation by the periodic inspection
• | Auto Learning Failure – 4 ID not learn in 19 minutes
• | Sensor Mute Failure - Not received frame for 17 minutes
• | RF IC Failure - 4 sensor mute DTC occurred and RF IC not respond
• | ECU Under/Over voltage – IG_ON < 9V for 2 sec or IG_ON > 16V for 2sec
• | EEPROM Failure – EEPROM IC not respond or CRC Check error
• | CAN Bus Failure
Warning Condition
• | Low Pressure