| VELOSTER(FS) >2013 > G 1.6 GDI > Fuel System > Fuel Delivery System > Fuel Filter>Repair procedures |

Replacement
1. | Remove the fuel pump (Refer to “Fuel Pump” in this group).
2. | Disconnect the electric pump wiring connector (A) and the fuel sender connector (B).
3. | Remove the head assembly (A) after releasing the cushion fixing clip (B).
4. | Disconnect the fuel tube quick-connectors (C).
5. | Remove the fuel sender (A) in the direction of an arrow.
6. | Disconnect the fuel tube connector (A).
7. | Remove the ORVR valve (A) after releasing hooks (B).
8. | Remove the reservior-cup (B) after releasing the fixing hooks (A).
9. | Release the fixing hooks, and then remove the pre-filter (A) and the fuel pressure regulator (B).
Be careful of O-ring.
10. | Replace new fuel filter. 1. Head assembly 2. Electric pump motor 3. Fuel filter 4. Fuel sender 5. Fuel pressure regulator 6. Pre-filter 7. Reservoir cup 8. ORVR valve