| VELOSTER(FS) >2013 > G 1.6 GDI > Body Electrical System > Smart key System > Smart key>Repair procedures |

Smart Key
Smart Key Code Saving
1. | Connect the DLC cable of GDS to the data link connector in driver side crash pad lower panel, turn the power on GDS.
2. | Select the vehicle model and then do "Smart key code saving".
3. | After selecting "Smart key teaching" menu, push "Enter" key, then the screen will be shown as below.
4. | After pushing the SSB with the teaching key, press "OK" button.
5. | Input the "Pin code" for first key teaching.
6. | Confirm the message "First key teaching completed".
7. | Confirm the message "Second key teaching completed".
8. | Then the screen will be shown as below when key teaching process is completed.