| VELOSTER(FS) >2013 > G 1.6 GDI > Restraint (Advanced) > SRSCM > Side Impact Sensor (SIS)>Repair procedures |

Removal
Pressure Side Impact Sensor
• | Removal of the airbag must be performed according to the precautions/procedures described previously.
• | Before disconnecting the side impact sensor connector(s), disconnect the side airbag connector(s).
• | Do not turn the ignition switch ON and do not connect the battery cable while replacing the side impact sensor.
1. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.
2. | Remove the front door trim. (Refer to the Body group - "Front door")
3. | Disconnect the pressure side impact sensor connector (A) and remove the pressure side impact sensor mounting screws (B).
Side Impact Sensor
1. | Disconnect the battery negative cable and wait for at least three minutes before beginning work.
2. | Remove the door scuff trim. (Refer to the Body group - "Interior trim")
3. | Remove the center pillar trim. (Refer to the Body group - "Interior trim")
4. | Disconnect the side impact sensor connector (A).
5. | Loosen the side impact sensor mounting bolt (B) and remove the side impact sensor.
Installation
Pressure Side Impact Sensor
1. | Install the new pressure side impact sensor with the screws (B) then connect the pressure side impact sensor connector (A).
Tightening torque : 1.1 ~ 1.3 N.m (0.11 ~ 0.13 kgf.m, 0.81 ~ 0.96 lb-ft)
• | Use the specified screws only.
2. | Install the front door trim. (Refer to the Body group - "Front door")
3. | Reconnect the battery negative cable.
4. | After installing the pressure side impact sensor, confirm proper system operation:
A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.
• | You must comply with the specified tightening torques with the tool specified because Pressure – Side Impact Sensors (P-SIS) may be broken or POP-NUT may be rotated.
• | Problems may be occurred in the durability of P-SIS or impact sensing performance may be depreciated if POP-NUT is rotated.
• | The door module must not be transformed because SRSCM judges a impact through the pressure sensor in the door module.
Side Impact Sensor
• | Do not turn the ignition switch ON and do not connect the battery cable while replacing the side impact sensor.
1. | Install the new side impact sensor with the bolt (B) then connect the side impact sensor connector (A).
Tightening torque: 7.0 ~ 9.0 N.m (0.71 ~ 0.92 kgf.m, 5.2 ~ 6.6 lb-ft)
2. | Install the center pillar trim. (Refer to the Body group - "Interior tirm")
3. | Install the door scuff trim. (Refer to the Body group - "Interior tirm")
4. | Reconnect the battery negative cable.
5. | After installing the Side Impact Sensor, confirm proper system operation:
A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.