| VELOSTER(FS) >2013 > G 1.6 GDI > Body Electrical System > Horn>Repair procedures |

Inspection
Test the horn by connecting battery voltage to the 1 terminal and ground the 2 terminal. The horn should make a sound. If the horn fails to make a sound, replace it. Horn Relay Inspection
1. | Remove the horn relay (A) from the engine room relay box.
2. | There should be continuity between the No.30 and No.87 terminals when power and ground are connected to the No.85 and No.86 terminals.
3. | There should be no continuity between the No.30 and No.87 terminals when power is disconnected.
Removal
1. | Remove the mounting bolt and disconnect the horn connector (B), then remove the horn (A).
Installation
1. | Connect the horn connector, then reassemble the horn.
Adjustment
Operate the horn, and adjust the tone to a suitable level by turning the adjusting screw.
After adjustment, apply a small amount of paint around the screw head to keep it from loosening.