| VELOSTER(FS) >2013 > G 1.6 GDI > Body Electrical System > Lighting System > Hazard Lamp Switch>Repair procedures |

Inspection
1. | The GDS will be able to diagnose defects of hazard switch quickly. The GDS can operates actuator manually, input/output value monitoring and self diagnosis.
2. | Select model and "BCM".
3. | Select the "SJB" to check.
4. | Select "Current data", if you will check current data of hazard switch. It provides input/output status of SJB.
Removal
1. | Disconnect the negative(-) battery terminal.
2. | Remove the heater control module. (Refer to the HA group - "Controller")
Installation
1. | Install the heater control module. (Refer to the HA group - "Controller")