| VELOSTER(FS) >2013 > G 1.6 GDI > Suspension System > Rear Suspension System > Rear Torsion Beam Axle>Repair procedures |

Replacement
1. | Remove the rear wheel & tire.
Tightening torque : 88.3 ~ 107.9N.m(9.0 ~ 11.0kgf.m, 65.1 ~ 79.6lb-ft)
Be careful not to damage to the hub bolts when removing the rear wheel & tire.
2. | Remove the parking brake bracket (A).
Tightening torque : 9.8 ~ 13.7N.m (1.0 ~ 1.4kgf.m, 7.2 ~ 10.1lb-ft)
3. | Loosen the bolt and then remove the wheel speed sensor cable (A) from the torsion beam axle.
Tightening torque : 6.9 ~ 10.8N.m(0.7 ~ 1.1kgf.m, 5.1 ~ 8.0lb-ft)
4. | Remove the brake caliper assembly (A) from the torsion beam axle by loosening the bolts.
Tightening torque : 63.7 ~ 73.5N.m(6.5 ~ 7.5kgf.m, 47.0 ~ 54.2lb-ft)
5. | Loosen the bolt & nut and then remove the rear shock absorber (A) from the torsion beam axle (B).
Tightening torque : 98.1 ~ 117.7N.m (10.0 ~ 12.0kgf.m, 72.3 ~ 86.8lb-ft)
6. | Remove the torsion beam axle (A) from the body loosening the bolts.
Tightening torque : 137.3 ~ 156.9N.m (14.0 ~ 16.0kgf.m, 101.3 ~ 115.7lb-ft)
7. | Remove the rear hub assembly. (Refer to DS group - "Rear Axle")
8. | Installation is the reverse of removal.