| VELOSTER(FS) >2013 > G 1.6 GDI > Body Electrical System > Keyless Entry And Burglar Alarm>Specifications |

Specification
Item | Description
Power source | 3V
Operating temperature | -20°C ~ +60°C
RF Modulation | FSK
LF Modulation | ASK
RF frequency | 315MHz
Battery | 1EA (CR2032)
Transmissible distance | 10m or more
Life of battery | 2years or more(at 20 times per day)
Button number | 3
Function | Door lock
Door unlock
Trunk lid open