| VELOSTER(FS) >2013 > G 1.6 GDI > Body Electrical System > Fuses And Relays > Relay Box (Passenger Compartment)>Repair procedures |

Fuse Inspection
1. | Be sure there is no play in the fuse holders, and that the fuses are held securely.
2. | Are the fuse capacities for each circuit correct?
3. | Are there any blown fuses? If a fuse is to be replaced, be sure to use a new fuse of the same capacity. Always determine why the fuse blew first and completely eliminate the problem before installing a new fuse.
Removal
Passenger Compartment Junction Box (IPM)
1. | Disconnect the negative(-) battery terminal.
2. | Remove the crash pad lower panel. (Refer to the BD group - "Crash pad")
3. | Disconnect the connectors from the fuse side of the passenger compartment junction box (A).
4. | Remove the passenger compartment junction box after loosening the mounting nuts (2EA) and bolt.
5. | Disconnect the connectors and the cables from the back side of the passenger compartment junction box.
Installation
1. | Install the connectors and the cables from the back side of the passenger compartment junction box.
2. | Install the crash pad lower panel.
3. | Check that all system operates normally.