| VELOSTER(FS) >2013 > G 1.6 GDI > Body (Interior and Exterior) > Bumper > Front Bumper>Repair procedures |

Replacement
• | Put on gloves to protect your hands.
• | Use a plastic panel removal tool to remove interior trim pieces to without marring the surface.
• | Take care not bend or scratch the cover and other parts.
1. | Loosen the radiator upper cover (A) mounting clips.
2. | After loosening the front bumper side’s mounting screw, then disconnect the side’s.
3. | Remove the front bumper lower mounting clips.
4. | Disconnect the fog lamp connector (A).
5. | Remove the front bumper.
6. | Installation is the reverse of removal.
• | Make sure the connector is plugged in properly.
• | Replace any damage clips.