| VELOSTER(FS) >2013 > G 1.6 GDI > Body (Interior and Exterior) > Exterior > Mirror>Repair procedures |

Replacement
Outside Rear View Mirror Replacement
• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Put on gloves to protect your hands.
1. | Using a screwdriver or remover, remove the front door quadrant inner cover (A).
2. | Disconnect the outside rear view mirror connector (A).
3. | After loosening the mounting bolts, then remove the outside rear view mirror (B).
Tightening torque : 3.9 ~ 5.9 N.m (0.4 ~ 0.6 kgf.m, 2.9 ~ 4.3 lb-ft)
4. | Installation is the reverse of removal.
Inside Rear View Mirror Replacement
1. | Loosen the mounting screw (C).
2. | Push the inside rear view mirror base (B) up to remove to inside rear view mirror assembly (A).
3. | Installation is the reverse of removal.
ECM Mirror Replacement
1. | Remove the ECM mirror cover (B).
2. | Disconnect the ECM mirror connector (A).
3. | Loosen the mounting screw (B), push the ECM mirror base up to remove the ECM mirror assembly (A).
4. | Installation is the reverse of removal.
• | Make sure the connector are connected in properly.