| VELOSTER(FS) >2013 > G 1.6 GDI > Heating,Ventilation, Air Conditioning > Air Conditioning System > Evaporator Temperature Sensor>Repair procedures |

Inspection
1. | Ignition "OFF".
2. | Remove the evaporator temperature sensor after disconnecting the connector.
3. | Using the multi-tester, measure resistance between terminal "+" and "-" of evaporator temperature sensor. Specification
Evaporator core temperature[°C(°F)] | Resistance[kΩ] | Voltage[V]
-20 (-4) | 13.59 | 2.88
-10 (14) | 6.273 | 1.927
0 (32) | 3.129 | 1.192
10 (50) | 1.668 | 0.715
20 (68) | 0.942 | 0.431
30 (86) | 0.56 | 0.265
40 (104) | 0.347 | 0.168
50 (122) | 0.224 | 0.11
Replacement
1. | Disconnect the negative (-) battery terminal.
2. | Disconnect the evaporator temperature sensor connector.
3. | Remove the evaporator temperature sensor (A), by pulling it after rotating 90° in a counterclockwise direction.
4. | Installation is the reverse order of removal.