| VELOSTER(FS) >2013 > G 1.6 GDI > Restraint (Advanced) > SRSCM > Passive Occupant Detection System (PODS-F)>Repair procedures |

Removal
PODS-F ECU
1. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.
2. | Remove the front passenger seat assembly. (Refer to the Body group - "Seat")
3. | Disconnect the PODS-F ECU connector.
4. | Remove the seat cushion cover assembly. (Refer to the Body group - "Seat")
5. | Remove the seat track assembly. (Refer to the Body group - "Seat")
PODS-F Mat
1. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.
2. | Remove the front passenger seat assembly. (Refer to the Body group - "Seat")
3. | Disconnect the PODS-F mat connector.
4. | Remove the seat cushion assembly. (Refer to the Body group - "Seat")
Installation
PODS-F ECU
1. | Install the PODS-F ECU equipped seat track assembly. (Refer to the Body group - "Seat")
2. | Install the seat cushion cover assembly. (Refer to the Body group - "Seat")
3. | Connect the PODS-F ECU connector.
4. | Install the front passenger seat assembly. (Refer to the Body group - "Seat")
5. | Reconnect the battery negative cable.
6. | After installing the PODS-F, confirm proper system operation :
A. | Turn the ignition switch ON the SRS indicator should be turned on for about six seconds and then go off.
B. | Telltale lamp will turn on for 4 seconds and be turned off for 3 seconds. After the 7 seconds, it shall remain off if the PODS-F does not require suppression and the passenger airbag is enabled.
Be sure to perform PODS-F reset with GDS after replcacing PODS-F equipped seat cushion.
PODS-F Mat
1. | Install the PODS-F Mat equipped seat cushion assembly. (Refer to the Body group - "Seat")
2. | Install the front passenger seat assembly. (Refer to the Body group - "Seat")
3. | Connect the PODS-F mat connector.
4. | Reconnect the battery negative cable.
5. | After installing the PODS-F, confirm proper system operation :
A. | Turn the ignition switch ON the SRS indicator should be turned on for about six seconds and then go off.
B. | Telltale lamp will turn on for 4 seconds and be turned off for 3 seconds. After the 7 seconds, it shall remain off if the PODS-F does not require suppression and the passenger airbag is enabled.
Be sure to perform PODS-F zeroing with GDS after replcacing PODS-F equipped seat cushion.
PODS-F Zeroing procedure
You should perform PODS-F Re-zero procedure after service or replacement about all part of the passenger seat. (Not included full seat assembly)
1. | Ignition “OFF”, connect GDS.
2. | Ignition “ON” & Engine “OFF”, select Airbag system and “PODS-F Reset” mode.
3. | The GDS will show the two PODS-F Zeroing function steps.
(1) | Erase PODS-F diagnostic codes.
(2) | PODS-F initialization.
This step must be done PODS-F re-zero, when the front passenger seat is empty.
4. | The PODS-F initialization procedure will be performed.
Erase the SRSCM diagnostic codes after completing the PODS-F zeroing.
In case of zeroing failure
- | Code 01 : Requestor ID out of range.
- | Code 02 : ECU faults.
- | Code 03 : ODS sensor short to ground.
- | Code 04 : Open between ODS ECU and mat.
- | Code 05 : ODS ECU has not been trimmed.
- | Code 06 : Configuration disabled in ECU calibration.
- | Code 07 : Configuration value out of range.
- | Code 08 : Used in zero Request response only.
- | Code 09 : Algo enabled this ignition cycles.
- | Code 0A : Upper offset value created during the zero process.
- | Code 0B : Lower offset value created during the zero process.
- | Code 0C : Voltage diagnostic
- | Code 0D : The delta of QX_Freq_Low and QX_Freq_High must remain low.
- | Code 0E : Temperature is above O deg C during the zero process.
- | Code 0F : Re-read QX Final compare delta limit. (zero verify)